;; net8192su.inf 
;;
;;

[Version]
Signature	= "$Chicago$"
Compatible	= 1
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= net8192su.cat		;; for WHQL certified
DriverVer = 11/04/2010,1084.44.1104.2010

[Manufacturer]
%Realtek% = Realtek, NTX86.5.1, NTamd64.5.1, NTX86.6.0, NTamd64.6.0, NTX86.6.1, NTamd64.6.1

[ControlFlags]
ExcludeFromSelect = *

[Realtek]

[Realtek.NTX86.5.1]
%RTL8188su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8171
%RTL8191su.DeviceDesc% = RTL8192su.ndi, USB\VID_0BDA&PID_8172

[Realtek.NTamd64.5.1]

[Realtek.NTX86.6.0]

[Realtek.NTamd64.6.0]

[Realtek.NTX86.6.1]

[Realtek.NTamd64.6.1]


;;****************************************************************************
;; Windows 2000/XP
;;****************************************************************************
;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------
[RTL8192su.ndi.NT]
AddReg			= RTL8192su.nt5.reg, RTL8192su.common.reg, RTLWLAN.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles

[RTL8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt5.Service, RTL8192su.nt5.EventLog

;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------
[RTLG8192su.ndi.NT]
AddReg			= RTL8192su.nt5.reg, RTL8192su.common.reg, RTLWLAN.reg, 11gWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles

[RTLG8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt5.Service, RTL8192su.nt5.EventLog

;;----------------------------------------------------------------------------
;; Corega customized installation
;;----------------------------------------------------------------------------
[Corega8192su.ndi.NT]
AddReg			= RTL8192su.nt5.reg, RTL8192su.common.reg, Corega.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles

[Corega8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt5.Service, RTL8192su.nt5.EventLog

;;----------------------------------------------------------------------------
;; EnGenius/Edimax customized installation
;;----------------------------------------------------------------------------
[CustWEP8192su.ndi.NT]
AddReg			= RTL8192su.nt5.reg, RTL8192su.common.reg, RTLWLAN.reg, WEPinGmode.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles

[CustWEP8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt5.Service, RTL8192su.nt5.EventLog

;;----------------------------------------------------------------------------
;; Dlink default installation
;;----------------------------------------------------------------------------
[Dlink8192su.ndi.NT]
AddReg			= RTL8192su.nt5.reg, RTL8192su.common.reg, RTLWLAN.reg, WEPinGmode.reg, 11nWirelessMode.reg
Characteristics		= 0x84
BusType			= 15 
CopyFiles		= RTL8192su.CopyFiles

[Dlink8192su.ndi.NT.Services]
AddService		= RTL8192su, 2, RTL8192su.nt5.Service, RTL8192su.nt5.EventLog

;;----------------------------------------------------------------------------
;; RTL8192su Parameters
;;----------------------------------------------------------------------------
;;****************************************************************************
;; Windows 2000/XP parameters
;;****************************************************************************
[RTL8192su.nt5.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "ethernet"
HKR, Ndi,		Service,    0, "RTL8192su"

[RTL8192su.nt5.Service]
DisplayName    = %RTL8192su.DeviceDesc.DispName%
ServiceType    = 1		; %SERVICE_KERNEL_DRIVER%
StartType      = 3		; %SERRVICE_DEMAND_START%
ErrorControl   = 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  = %12%\RTL8192su.sys
LoadOrderGroup = NDIS

[RTL8192su.nt5.EventLog]
AddReg = RTL8192su.nt5.AddEventLog.reg

[RTL8192su.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; RTL8192su common paramters
;*******************************************************************************
[RTL8192su.common.reg]
HKR,defaults,		   AH_BcnIntv, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 	0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 	0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 	0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 	0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 	0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 	0, "1"

; For PSP XLink mode, 2006.09.04, by shien chang.
HKR,Ndi\params\PSPXlinkMode,        ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,        type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,        default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

HKR,,LedCtrl,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,,Channel,0,"10"

HKR,Ndi\params\Dot11dEnable,        ParamDesc,  0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable,        type,       0, "enum"
HKR,Ndi\params\Dot11dEnable,        default,    0, "0"
HKR,Ndi\params\Dot11dEnable\enum,   "0",        0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum,   "1",        0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"

;;----------------------------------------------------------------------------
;; Corega WLAN NIC parameters
;;----------------------------------------------------------------------------
[Corega.reg]
HKR,Ndi\params\Channel,       ParamDesc,  0, %CHANNEL_STR%
HKR,Ndi\params\Channel,       type,       0, "int"
HKR,Ndi\params\Channel,       default,    0, "1"
HKR,Ndi\params\Channel,       Min,        0, "1"
HKR,Ndi\params\Channel,       Max,        0, "13"
HKR,Ndi\params\Channel,       Step,       0, "1"
HKR,Ndi\params\Channel,       Base,       0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,,TKIPinNmode,0,"1"

;;----------------------------------------------------------------------------
;; EnGenius WLAN NIC parameters
;;----------------------------------------------------------------------------
[WEPinGmode.reg]
HKR,,WEPinNmode,0,"0"

;;----------------------------------------------------------------------------
;; Wireless mode option parameters
;;----------------------------------------------------------------------------
[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,WirelessBgSku,0,"1"

[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"


;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTL8192su.CopyFiles]
RTL8192su.sys,,,2

[DestinationDirs]
RTL8192su.CopyFiles	= 12

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
RTL8192su.sys = 1

[SourceDisksNames]
1=%DISKNAME%,,,

;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
Realtek 			= " "
SSID_STR			= "SSID"
CHANNEL_STR			= "Channel"
NETWORK_TYPE_STR		= "Network Type"
LED_CONTROL_STR			= "LED Control" 
POWER_SAVE_STR			= "Power Save Mode"
WIFI_IBSS_STR			= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR		= "Rate Adaptive"
QOS_STR				= "QoS"
WMM_APSD			= "WMM APSD"
CCX_RM_STR			= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR	= "CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR		= "Forced Priority"
HW_PARA_STR			= "Init from HwParaFile"
THREE_WIRE_MODE_STR		= "Three Wire Programming Mode"
BOARD_TYPE_STR			= "Board Type"
PROTECTION_MODE_STR		= "Protection Mode"
TPC_STR				= "Transmit Power Control"
TPC_POLARITY_STR		= "TPC Polarity Select"
HIGH_POWER_STR			= "High Power Mechanism"
INIT_GAIN_STR			= "Initial Gain State"
CW_MAX_MIN_STR			= "Contention Window"
PSP_XLINK_STR			= "PSP XLink Mode"
DOT11_ENABLE_STR 		= "802.11d"
AH_BCNINTV_STR 			= "Beacon Interval"
DISABLE_STR 			= "Disable"
ENABLE_STR 			= "Enable"
WL_MODE_STR			= "Wireless Mode"
IEEE_802_11B_STR 		= "IEEE 802.11b"
IEEE_802_11BG_STR 		= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 		= "IEEE 802.11b/g/n"
TX_PWR_CONTROL_STR		= "Tx Power Control"
TX_PWR_PERCENTAGE_1_STR 	= "12.5%"
TX_PWR_PERCENTAGE_2_STR 	= "25%"
TX_PWR_PERCENTAGE_3_STR 	= "50%"
TX_PWR_PERCENTAGE_4_STR 	= "100%"

;; Source disk name
DISKNAME			= "Wireless Lite N Adapter Driver Disk"
RTL8188su.DeviceDesc 		= "Wireless Lite N Adapter"
RTL8188su.DeviceDesc.DispName	= "Wireless Lite N Adapter"
RTL8191su.DeviceDesc 		= "Wireless Lite N Adapter"
RTL8191su.DeviceDesc.DispName	= "Wireless Lite N Adapter"
RTL8192gu.DeviceDesc 		= "Wireless Lite N Adapter"
RTL8192gu.DeviceDesc.DispName	= "Wireless Lite N Adapter"
RTL8192su.DeviceDesc 		= "Wireless Lite N Adapter"
RTL8192su.DeviceDesc.DispName	= "Wireless Lite N Adapter 8191su"
RTL8712.DeviceDesc 		= "Wireless Lite N Adapter"
RTL8712.DeviceDesc.DispName	= "Wireless Lite N Adapter"